Solmeta GMAX (for Nikon cameras) Firmware Ver2.5 (201605181107-Release)

The new firmware file name is ¡°GMAX_for_Nikon_Ver2.5_201605181107-Release.dfu¡±

The Ver 2.5 is an upgrade firmware from Ver 2.3 (201602021739-Release). 
Some changes, improvements and fixes.
1.Fixed a problem regarding the compatibility of GMAX and Nikon D810.
( many thanks to great user named Mr. Bradford Glade in USA )
2.Improve the Timer release minimum interval time from 4 sec. to 3 sec. The improvement provides aerial photography user shooting interval as fast as possible. 
3.The air pressure unit changes to inHg instead of PSI. Also, user can use inHg unit to do ¡°Sea-Leavel Calibration¡± directly.
4.To support more application, the data format for information of D-GPS is masked into normal data format in the GMAS¡¯s log files. 

When doing the firmware upgrade, please read the information bellow thoroughly.
1.To do the firmware upgrade, please refer to the guide of GMAX_Firmware_upgrading_guide.pdf in the folder.
2.The tools program supports 32Bit Windows system. The best is Windows7 32bit.

If you use MAC OSX, you need to download ¡°DfuSe¡± burning chip tool and driver by yourself.  If you install the firmware and try to run the DfuSe Demo software, sometimes it might immediately fail with the following error:
 "The application was unable to start correctly (0xc0150002). Click OK to close the application."
In this case you determine that the software was depending on ¡°Visual Studio 2005 Service Pack 1 Redistributable Package MFC Security Update¡±. Once you install that you are able to run the software and can see the GMAX as a device to upgrade. 


SOLMETA CO., LTD
May 18, 2016


